OLED Customization Request Form

	Company Name :
	Country :
	Date :

	Application :
	End User :

	EAU :
	Project Duration :

	Target Price (USD) :

	Est. Sample Require date :

	Est. Mass Production Require date :

	Project :
	· New Design
	· Replaced 
	· TBD/Other :

	Ref. Drawing
	· No
	· Yes, see attached file            "following omitted."
	· TBD/Other :

	Existing Panel:
	· No
	· Yes, module Serial :                "following omitted."
	· TBD/Other :

	Structure :
	· COB
	· TAB
	· COG
	· TBD/Other :

	Style :
	□ Graphic:    x    dots
	□ Character:     C x    L
	□ ICON:    icons
	· TBD/Other :

	
	· TOLED  □ PMOLED
	· Hole punched  size : 
	· TBD/Other :

	Outline :
	Length(mm):
	Width(mm):
	· TBD/Other :

	View area :
	Length(mm):
	Width(mm):
	· TBD/Other :

	Active area :
	Length(mm):
	Width(mm):
	· TBD/Other :

	Dot size :
	Length(mm):       (min 0.1mm)
	Width(mm):          (min 0.1mm)
	· TBD/Other :

	Dot pitch :
	Length(mm):      (min 0.12mm)
	Width(mm):        (min 0.12min )
	· TBD/Other :

	Color :
	· Yellow
	· Green
	· White
	· Skyblue
	· TBD/Other :

	
	CIE-X: 
	CIE-Y:
	· TBD/Other :

	Glass thickness
	□ 1.8mm (default)
	□ 1.4mm
	□ 1.2mm
	· TBD/Other :

	Polarizer :
	· N/A
	· Regular
	· Anti-glare
	· Anti-UV
	· TBD/Other :

	Connect type :
	· FPC
□ Hot Bar
□ Pin
□ Cable
	□Pin number :
	□SMT
	· TBD/Other :

	
	
	□Pin pitch(mm):         
(FPC 0.5/1.0) / (HOT Bar 0.62/0.7)
	

	
	
	□FPC length(mm):              
(guarantee min 12mm)
	

	
	
	□Bent,  r =    mm           
(guarantee min = 2 mm)
	

	
	· TBD / Other :

	Fixed structure
	□ N/A
	□ Metal frame

	□ Plastic frame
	· PCB
	· TBD/Other :


	Cover glass
	□ Tempered glass  
	□ PMMA
	Ink color 

	
	□ Semi-transmissive    T % =

	
	[bookmark: _GoBack]□ OCA bonding    □ Air bonding   □ TBD/Other :



	Touch Integrated 
	· NA 
	· Resistive
	· Capacitive

	
	· Touch key   (     keys)
	
	

	Description :
	□ Industrial grade (default)
	□ Consumer grade

	
	□ □ Charge pump built-in

	
	· Wide temperature
	High:    ℃ ~ Low:    ℃
	(Default:-40℃ ~ 80℃)

	
	· Other

	Special requirements :
	· Lifetime(HRS) :
	· Appointed IC:

	
	□ Brightness(cd/㎡) :
	· Appointed interface:

	
	□ Logic supply voltage :
	□ 3V
	□ 5V

	
	□ Final product ESD test  (Please provide attachments detailing the specifications and measure method.)

	
	□ Final product mechanical test  (Please provide attachments detailing the specifications and measure method.)

	
	□ Other designated reliability verification items (Please provide attachments detailing the specifications and measure method.)
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